{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-B"]
[]
[]
[]
[]
["","","","","FTXA50C2V1BW / RXA50B5V1B","FTXA50C2V1BW / RXA50B2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.70","1.70"]
["","Ονομ.","","kW","5.00","5.00"]
["","Μέγ.","","kW","5.30","5.30"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.70","1.70"]
["","Ονομ.","","kW","5.80","5.80"]
["","Μέγ.","","kW","6.50","6.50"]
["Ονομαστική απόδοση","EER","","","3.68","3.68"]
["","COP","","","4.00","4.00"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","679","679"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++"]
["","Απόδοση","Pdesign","kW","5.00","5.00"]
["","SEER","","","7.33","7.33"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","239","239"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++"]
["","Απόδοση","Pdesign","kW","4.00","4.00"]
["","SCOP/A","","","4.60","4.60"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","3.19","3.19"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","1218","1218"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","A+++ ~ D"]
["Σημειώσεις","","","","","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]