{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":14,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B","FTXF20A2V1B (Archived)","FTXF20A5V1B (Archived)","FTXF25A2V1B (Archived)","FTXF25A5V1B (Archived)","FTXF35A2V1B (Archived)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","40","","","","39","39","40","40","40"]
["","","","Μέτρια","dBA","35","","","","34","34","34","34","35"]
["","","","Αθόρυβη λειτουργία","dBA","21","","","","21","21","21","21","21"]
["","","","Χαμηλή","dBA","29","","","","28","28","28","28","29"]
["","Ψύξη","","Μέτρια","dBA","34","","","","33","33","33","33","34"]
["","","","Αθόρυβη λειτουργία","dBA","20","","","","20","20","20","20","20"]
["","","","Χαμηλή","dBA","27","","","","25","25","26","26","27"]
["","","","Υψ.","dBA","43","","","","39","39","40","40","43"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","","","","1","1","1","1","1"]
["","Εγχειρίδιο χειρισμού","","","","1","","","","1","1","1","1","1"]
["","Τηλεχειριστήριο υπερύθρων","","","","1","","","","1","1","1","1","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2","","","","2","2","2","2","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","","","","1","1","1","1","1"]
["","Πλάκα στήριξης","","","","1","","","","1","1","1","1","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2","","","","2","2","2","2","2"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","","","","6.35","6.35","6.35","6.35","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50","","","","9.50","9.50","9.50","9.50","9.50"]
["","Συμπυκνωμάτων","","","","18","","","","18","18","18","18","18"]
["Power input","Ψύξη","","Ονομ.","kW","0.032","","","","0.017","0.017","0.019","0.019","0.032"]
["","Θέρμανση","","Ονομ.","kW","0.032","","","","0.020","0.020","0.020","0.020","0.032"]
["Sound power level","Ψύξη","","","dBA","58","","","","55","55","55","55","58"]
["","Θέρμανση","","","dBA","58","","","","55","55","55","55","58"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","770","","","","770","770","770","770","770"]
["","","","Βάθος","mm","225","","","","225","225","225","225","225"]
["","","","Ύψος","mm","286","","","","286","286","286","286","286"]
["Περίβλημα","Χρώμα","","","","Λευκό","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","","kg","9.00","","","","9.00","9.00","9.00","9.00","9.00"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","11.5","","","","10.3","10.3","10.3","10.3","11.5"]
["","","","Χαμηλή","m³/min","7.0","","","","6.5","6.5","6.7","6.7","7.0"]
["","","","Μέτρια","m³/min","9.0","","","","8.4","8.4","8.6","8.6","9.0"]
["","","","Αθόρυβη λειτουργία","m³/min","5.3","","","","5.3","5.3","5.3","5.3","5.3"]
["","","Ψύξη","Χαμηλή","m³/min","6.3","","","","5.9","5.9","6.1","6.1","6.3"]
["","","","Μέτρια","m³/min","8.3","","","","7.9","7.9","8.1","8.1","8.3"]
["","","","Υψ.","m³/min","11.5","","","","9.8","9.8","10.1","10.1","11.5"]
["","","","Αθόρυβη λειτουργία","m³/min","4.5","","","","4.4","4.4","4.4","4.4","4.5"]
["Power supply","Φάση","","","","1~","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","","","","50","50","50","50","50"]
["","Τάση","","","V","220-240","","","","220-240","220-240","220-240","220-240","220-240"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.029","0.032","0.032"]
["","Θέρμανση","","Ονομ.","kW","","0.032","0.035","0.035"]
["Περίβλημα","Χρώμα","","","","","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","295","295","295"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","990","990","990"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","263","263","263"]
["Βάρος","Μονάδα","","","kg","","13.5","13.5","13.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","16.8","17.3","17.3"]
["","","","Μέτρια","m³/min","","14.4","14.8","14.8"]
["","","","Χαμηλή","m³/min","","11.9","12.2","12.2"]
["","","","Αθόρυβη λειτουργία","m³/min","","10.5","10.7","10.7"]
["","","Θέρμανση","Υψ.","m³/min","","17.3","17.9","17.9"]
["","","","Μέτρια","m³/min","","14.8","15.8","15.8"]
["","","","Χαμηλή","m³/min","","12.2","12.8","12.8"]
["","","","Αθόρυβη λειτουργία","m³/min","","10.7","11.3","11.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","59","60","62"]
["","Θέρμανση","","","dBA","","61","62","62"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","43","45","46"]
["","","","Μέτρια","dBA","","39","41","42"]
["","","","Χαμηλή","dBA","","34","36","37"]
["","","","Αθόρυβη λειτουργία","dBA","","31","33","34"]
["","Θέρμανση","","Υψ.","dBA","","42","44","45"]
["","","","Μέτρια","dBA","","38","40","41"]
["","","","Χαμηλή","dBA","","33","35","36"]
["","","","Αθόρυβη λειτουργία","dBA","","30","32","33"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","12.7","12.7","12.7"]
["","Αποχέτευση","","","","","18","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Τηλεχειριστήριο με καλώδιο","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2"]
["","Operation manual","","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","2","2"]
["","Indoor unit fixing screws","","","","","2","2","2"]
["","Infrared remote control","","","","","1","1","1"]
["","Mounting plate","","","","","1","1","1"]
["","Remote control holder","","","","","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","V1","V1","V1"]
["","Φάση","","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50"]
["","Τάση","","","V","","220-240","220-240","220-240"]