{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B / RXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B / RXF20B5V1B","FTXF25B5V1B / RXF25B5V1B"]
["Outdoor unit","","","","RXF20B5V1B","RXF25B5V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.3","1.3"]
["","Ονομ.","","kW","2.00","2.50"]
["","Μέγ.","","kW","2.6","3.0"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.30","1.30"]
["","Ονομ.","","kW","2.50","2.80"]
["","Μέγ.","","kW","3.50","4.00"]
["Ονομαστική απόδοση","EER","","","3.94","3.30"]
["","COP","","","4.19","4.01"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++"]
["","Απόδοση","Pdesign","kW","2.00","2.50"]
["","SEER","","","6.15","6.22"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","114","141"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A+"]
["","Απόδοση","Pdesign","kW","2.20","2.40"]
["","SCOP/A","","","4.10","4.06"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","1.99","2.10"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","751","827"]
["Εύρος ενεργειακής αποδοτικότητας","","","","A+++ ~ D","A+++ ~ D"]