{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-C"]
[]
[]
[]
[]
["","","","","","FTXF20C5V1B","FTXF25C5V1B","FTXF35C5V1B","FTXF42C5V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.023","0.023","0.029","0.04"]
["","Θέρμανση","","Ονομ.","kW","0.023","0.023","0.029","0.04"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","286","286","286","286"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","770","770","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","225","225","225","225"]
["Βάρος","Μονάδα","","","kg","8","8","8.5","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","8.3","8.5","11.8","12.6"]
["","","","Μέτρια","m³/min","6","6","8","9"]
["","","","Χαμηλή","m³/min","4.6","4.6","6.4","6.9"]
["","","","Αθόρυβη λειτουργία","m³/min","3.6","3.6","4.4","4.9"]
["","","Θέρμανση","Υψ.","m³/min","9.7","9.7","11.9","12.8"]
["","","","Μέτρια","m³/min","7.8","7.9","8.6","8.8"]
["","","","Χαμηλή","m³/min","5.8","6","6.5","6.7"]
["","","","Αθόρυβη λειτουργία","m³/min","4.6","4.6","5.3","5.2"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53","54","54","59"]
["","Θέρμανση","","","dBA","55","55","56","59"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39","40","43","45"]
["","","","Μέτρια","dBA","33","33","34","36"]
["","","","Χαμηλή","dBA","25","26","27","30"]
["","","","Αθόρυβη λειτουργία","dBA","20","20","20","22"]
["","Θέρμανση","","Υψ.","dBA","39","40","40","44"]
["","","","Μέτρια","dBA","34","34","35","34"]
["","","","Χαμηλή","dBA","28","28","29","28"]
["","","","Αθόρυβη λειτουργία","dBA","21","21","21","22"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","6.35","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.5","9.5","9.5","9.5"]
["","Αποχέτευση","","","","18","18","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Τάση","","","V","220-440","220-440","220-440","220-440"]