{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXG-L"]
[]
[]
[]
[]
["","","","","FTXG20LV1BW / RXG20L2V1B","FTXG25LV1BW / RXG25L2V1B","FTXG35LV1BW / RXG35L2V1B","FTXG50LV1BW / RXG50L2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.3","1.3","1.4","1.7"]
["","Μέγ.","","kW","2.8","3.0","3.8","5.3"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.3","1.3","1.4","1.7"]
["","Μέγ.","","kW","4.3","4.5","5.0","6.5"]
["Ονομαστική απόδοση","EER","","","4.59","4.59","3.97","3.53"]
["","COP","","","5.00","4.42","4.06","3.65"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","250.5","261.5","441","680"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A","A"]
["","","Θέρμανση","","A","A","A","A"]
["Συνδέσεις σωληνώσεων","Συμπυκνωμάτων","Εξ.Διάμ.","χιλ.","18","18.0","18.0","18.0"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","χιλ.","9.5","9.5","9.5","12.7"]
["","Υγρό","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","6.35","6.35","6.35"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A+++","A+++","A++","A++"]
["","Απόδοση","Pdesign","kW","2.30","2.40","3.50","4.80"]
["","SEER","","","8.52","8.50","7.00","6.70"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","94","99","175","251"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++","A++","A+"]
["","Απόδοση","Pdesign","kW","2.10","2.70","3.00","4.60"]
["","SCOP/A","","","4.60","4.60","4.60","4.24"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","639","821","913","1519"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]