{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","7.50"]
["Ψύξη χώρου","SEER","","","6.92"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","380"]
["","Απόδοση","Pdesign","kW","7.50"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A++"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","2,245"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","908"]
["","EER","","","4.13"]
["","COP","","","3.32"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","C"]
["Απόδοση θέρμανσης","Ονομ.","","kW","10.00"]
["Σημειώσεις","","","","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]