{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXK-AW"]
[]
[]
[]
[]
["","","","","FTXK25AV1BW","FTXK35AV1BW","FTXK50AV1BW","FTXK60AV1BW"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","40","41","40","43"]
["","","Αθόρυβη λειτουργία","dBA","21","22","32","33"]
["","","Χαμηλή","dBA","29","30","35","37"]
["","Ψύξη","Αθόρυβη λειτουργία","dBA","21","22","32","33"]
["","","Υπερ-υψηλό","dBA","41","42","44","46"]
["","","Χαμηλή","dBA","29","30","35","37"]
["","","Υψ.","dBA","40","41","40","43"]
["","","Ονομ.","dBA","34","34","38","41"]
["","Ψύξη","Ονομ.","dBA","34","34","38","41"]
["Ψυκτικό μέσο","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","12.70","15.90"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","53","54","55","61"]
["","Θέρμανση","","dBA","53","54","55","61"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","890","890","1,172","1,172"]
["","","Βάθος","mm","210","210","242","242"]
["","","Ύψος","mm","297","297","320","320"]
["Περίβλημα","Colour","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["Βάρος","Μονάδα","","kg","9.0","9.0","14.0","14.0"]
["Power supply","Φάση","","","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50","50","50","50"]
["","Όνομα","","","V1","V1","V1","V1"]
["","Τάση","","V","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)"]
["","","","","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση."]