{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-K / RXM-L"]
[]
[]
[]
[]
["","","","","FTXM20K3V1B / RXM20LV1B","FTXM25K3V1B / RXM25LV1B","FTXM35K3V1B / RXM35LV1B","FTXM42K3V1B / RXM42LV1B","FTXM50K3V1B / RXM50LV1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.30","1.30","1.40","1.70","1.70"]
["","Μέγ.","","kW","2.80","3.20","4.00","5.00","5.30"]
["","Ονομ.","","kW","2.00 (2)","2.50 (2)","3.50 (2)","4.20 (2)","5.02 (2)"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","9.5","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","18.0","18.0","18","18","18"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","221","288","428","607","738"]
["","EER","","","4.53 (1)","4.34 (1)","4.09 (1)","3.46 (1)","3.40 (1)"]
["","COP","","","4.55 (1)","4.52 (1)","4.76 (1)","4.12 (1)","4.00 (1)"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A","A","A"]
["","","Θέρμανση","","A","A","A","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","2.50 (2)","2.80 (2)","4.00 (2)","5.40 (2)","5.80 (2)"]
["","Ελάχ.","","kW","1.30","1.30","1.40","1.70","1.70"]
["","Μέγ.","","kW","4.30","4.70","5.20","6.00","6.50"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","","(3) - 220V","(3) - 220V","(3) - 220V","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V","(4) - 230V","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V","(5) - 240V","(5) - 240V","(5) - 240V"]