{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":11,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N"]
[]
[]
[]
[]
["","","","","","FTXP35N5V1B","FTXP50N2V1B","FTXP60N2V1B","FTXP71N2V1B","FTXP20N5V1B (Archived)","FTXP25N5V1B (Archived)"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.032","0.029","0.032","0.032","0.019","0.02"]
["","Θέρμανση","","Ονομ.","kW","0.032","0.032","0.035","0.035","0.023","0.023"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","286","295","295","295"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770","990","990","990"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","225","263","263","263"]
["Βάρος","Μονάδα","","","kg","9","13.5","13.5","13.5","8.5","8.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","11.5","16.3","16.8","16.8","9.5","9.7"]
["","","","Μέτρια","m³/min","8.3","14","14.4","14.4","7.4","7.7"]
["","","","Χαμηλή","m³/min","6.3","11.5","11.8","11.8","5.6","5.8"]
["","","","Αθόρυβη λειτουργία","m³/min","4.5","8.3","9.2","10.1","4.2","4.2"]
["","","Θέρμανση","Υψ.","m³/min","11.5","17.3","17.9","17.9","10.4","10.4"]
["","","","Μέτρια","m³/min","9","14.4","15.3","15.3","8.1","8.1"]
["","","","Χαμηλή","m³/min","7","11.8","12.4","12.4","6.2","6.4"]
["","","","Αθόρυβη λειτουργία","m³/min","5.3","10.4","11","11","5.2","5.2"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","58","59","60","62","55","55"]
["","Θέρμανση","","","dBA","58","61","62","62","55","55"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","43","43","45","46","39","40"]
["","","","Μέτρια","dBA","34","39","41","42","33","33"]
["","","","Χαμηλή","dBA","27","34","36","37","25","26"]
["","","","Αθόρυβη λειτουργία","dBA","20","27","30","32","19","19"]
["","Θέρμανση","","Υψ.","dBA","40","42","44","45","39","40"]
["","","","Μέτρια","dBA","35","38","40","41","34","34"]
["","","","Χαμηλή","dBA","29","33","35","36","28","28"]
["","","","Αθόρυβη λειτουργία","dBA","21","30","32","33","21","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6","6.4","6.4","6.4"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","12.7","12.7","12.7"]
["","Αποχέτευση","","","","18","18","18","18","18","18"]
["Χειριστήρια","Infrared remote control","","","","ARC480A78","ARC480A53","ARC480A53","ARC480A53"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","General safety precautions","","","","1","","","","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","V1","V1","V1"]
["","Φάση","","","","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Στάνταρτ εξαρτήματα","WLAN adapter kit","","","","","1","1","1"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","","","","286","286"]
["","","","Πλάτος","mm","","","","","770","770"]
["","","","Βάθος","mm","","","","","225","225"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","","","","6","6"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","","","","9.5","9.5"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","","","ARC480A78","ARC480A78"]
["Σημειώσεις","","","","","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m"]
["","","","","","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)"]
["","","","","","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]