{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":9,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9"]
[]
[]
[]
[]
["","","","","","FTXP25N5V1B9","FTXP35N5V1B9","FTXP50N5V1B9","FTXP20N5V1B9 (Archived)"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.023","0.032","0.04","0.021"]
["","Θέρμανση","","Ονομ.","kW","0.023","0.032","0.04","0.023"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","286","286","286"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","770","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","225","225","225"]
["Βάρος","Μονάδα","","","kg","9","9","9","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.9","11.5","11.8","9.6"]
["","","","Μέτρια","m³/min","7.5","8.3","9.3","7.5"]
["","","","Χαμηλή","m³/min","5.8","6.3","7.6","5.6"]
["","","","Αθόρυβη λειτουργία","m³/min","4.4","4.5","6","4.4"]
["","","Θέρμανση","Υψ.","m³/min","10.6","11.5","11.9","10.6"]
["","","","Μέτρια","m³/min","8.6","9","9.5","8.6"]
["","","","Χαμηλή","m³/min","6.6","7","8.2","6.6"]
["","","","Αθόρυβη λειτουργία","m³/min","5","5.1","7.4","5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","58","59","55"]
["","Θέρμανση","","","dBA","55","58","61","55"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","40","43","46","39"]
["","","","Μέτρια","dBA","33","34","39","33"]
["","","","Χαμηλή","dBA","26","27","34","25"]
["","","","Αθόρυβη λειτουργία","dBA","19","20","27","19"]
["","Θέρμανση","","Υψ.","dBA","40","40","44","39"]
["","","","Μέτρια","dBA","34","35","38","34"]
["","","","Χαμηλή","dBA","28","29","33","28"]
["","","","Αθόρυβη λειτουργία","dBA","21","21","30","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","9.52","12.7"]
["","Αποχέτευση","","","","18","18","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC480A78","ARC480A78","ARC480A78","ARC480A78"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m"]
["","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)"]
["","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Διαστάσεις","Μονάδα","","Ύψος","χιλ.","","","","286"]
["","","","Πλάτος","χιλ.","","","","770"]
["","","","Βάθος","χιλ.","","","","225"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","χιλ.","","","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","χιλ.","","","","9.52"]