{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Στάθμη ηχ. πίεσης","Θέρμανση","","Υψ.","dBA","38","39","42","42","44","","46"]
["","","","Αθόρυβη λειτουργία","dBA","25","25","26","30","31","","34"]
["","","","Χαμηλή","dBA","28","28","29","33","34","","37"]
["","Ψύξη","","Αθόρυβη λειτουργία","dBA","22","22","23","30","31","","34"]
["","","","Χαμηλή","dBA","25","25","26","33","34","","37"]
["","","","Υψ.","dBA","38","38","42","42","43","","46"]
["","","","Ονομ.","dBA","33","34","36","38","39","","42"]
["","Ψύξη","","Ονομ.","dBA","32","32","34","38","39","","42"]
["Στάνταρτ εξαρτήματα","Φωτοκαταλυτικό φίλτρο αέρα από τιτάνιο με επικάλυψη απατίτη.","","","","2","2","2","2","2"]
["","Εγχειρίδιο χειρισμού","","","","1","1","1","1","1","","1"]
["","Εγχειρίδιο εγκατάστασης","","","","1","1","1","1","1","","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1","1","1","1","1","","1"]
["","Μπαταρίες","","","","2","2","2","2","2","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","1","1","1","1","","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2","2","2","2","2","","2"]
["","Πλάκα στήριξης","","","","1","1","1","1","1","","1"]
["Συστήματα ελέγχου","Infrared remote control","","","","","","","","","","ARC452A3"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Αερίου","","Εξ.Διάμ.","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Drain","","","","18","18","18","18","18","","18"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Θέρμανση","","Ονομ.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","54","54","58","58","59","","63"]
["","Θέρμανση","","","dBA","54","55","58","58","60","","62"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","800","800","800","800","800","","1,050"]
["","","","Βάθος","mm","215","215","215","215","215","","250"]
["","","","Ύψος","mm","295","295","295","295","295","","290"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό","","Λευκό"]
["Βάρος","Μονάδα","","","kg","9","9","10","10","10","","12"]
["Power supply","Φάση","","","","1~","1~","1~","1~","1~","","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","","50"]
["","Όνομα","","","","V1","V1","V1","V1","V1","","V1"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","","","","","","16.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","","","","","","41"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Ονομ.","m³/min","","","","","","14.9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","","","","","","40"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Θέρμανση","","Ονομ.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Περίβλημα","Χρώμα","","","","","","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","","","","","290"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","","","","","1050"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","","","","","250"]
["Βάρος","Μονάδα","","","kg","","","","","","12"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","","","","16.0"]
["","","","Χαμηλή","m³/min","","","","","","11.3"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","","","10.1"]
["","","Θέρμανση","Υψ.","m³/min","","","","","","17.2"]
["","","","Χαμηλή","m³/min","","","","","","12.6"]
["","","","Αθόρυβη λειτουργία","m³/min","","","","","","11.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","","","","60"]
["","Θέρμανση","","","dBA","","","","","","59"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","","","45"]
["","","","Χαμηλή","dBA","","","","","","36"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","","33"]
["","Θέρμανση","","Υψ.","dBA","","","","","","44"]
["","","","Χαμηλή","dBA","","","","","","35"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","","32"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","","","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","","","","12.7"]
["","Αποχέτευση","","","","","","","","","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","","","","ARC452A3"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Τροφοδοσία ισχύος","Όνομα","","","","","","","","","V1"]
["","Φάση","","","","","","","","","1~"]
["","Συχνότητα","","","Hz","","","","","","50"]
["","Τάση","","","V","","","","","","220-240"]
["Στάνταρτ εξαρτήματα","Φωτοκαταλυτικό φίλτρο καθαρισμού αέρα από τιτάνιο με επικάλυψη απατίτη χωρίς πλαίσιο","","","","","","","","","","2"]
["Σημειώσεις","","","","","","","","","","","(4) - 240V"]