{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L2V1B","FTXS25K2V1B / RXS25L2V1B","FTXS35K2V1B / RXS35L2V1B","FTXS42K2V1B / RXS42L2V1B","FTXS42K3V1B / RXS42L2V1B","FTXS50K2V1B / RXS50L2V1B","FTXS50K3V1B / RXS50L2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.3","1.3","1.4","1.7","1.7","1.7","1.7"]
["","Μέγ.","","kW","2.8","3.2","4.0","5.0","5.0","5.3","5.3"]
["","Ονομ.","","kW","2.00","2.5","3.5","4.20","4.20 (2)","5.00","5.00 (2)"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Αερίου","Εξ.Διάμ.","mm","9.5","9.5","9.5","9.5","12.7","12.7","12.7"]
["","Drain","OD","mm","18","18","18","18","18","18","18"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","215","285","430","590","627","705","753"]
["","EER","","","4.65","4.39","4.07","3.56","3.35 (1)","3.55","3.32 (1)"]
["","COP","","","4.72","4.67","4.76","4.12","4.12 (1)","4.00","4.00 (1)"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A","A","A","A","A"]
["","","Θέρμανση","","A","A","A","A","A","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","2.5","2.8","4.00","5.40","5.40 (2)","5.80","5.80 (2)"]
["","Ελάχ.","","kW","1.3","1.3","1.4","1.7","1.7","1.7","1.7"]
["","Μέγ.","","kW","4.3","4.7","5.2","6.0","6.0","6.5","6.5"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - 220V","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 220V","(3) - 230V","(3) - 220V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 230V","(4) - 240V","(4) - 230V"]
["","","","","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(5) - 240V","(5) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(5) - 240V"]