{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.029","0.053"]
["","Θέρμανση","","Ονομ.","kW","0.024","0.06"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","298","298"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","804","997"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","252","292"]
["Βάρος","Μονάδα","","","kg","12","15"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","13.2","15.1"]
["","","","Μέτρια","m³/min","8.1","9.2"]
["","","","Χαμηλή","m³/min","5.6","5.6"]
["","","","Αθόρυβη λειτουργία","m³/min","4.8","4.8"]
["","","Θέρμανση","Υψ.","m³/min","11.7","17"]
["","","","Μέτρια","m³/min","7.7","10"]
["","","","Χαμηλή","m³/min","5.6","6"]
["","","","Αθόρυβη λειτουργία","m³/min","4.7","5.1"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","60","60"]
["","Θέρμανση","","","dBA","59","60"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","45","46"]
["","","","Μέτρια","dBA","33","32"]
["","","","Χαμηλή","dBA","25","24"]
["","","","Αθόρυβη λειτουργία","dBA","21","20"]
["","Θέρμανση","","Υψ.","dBA","43","46"]
["","","","Μέτρια","dBA","31","31"]
["","","","Χαμηλή","dBA","22","22"]
["","","","Αθόρυβη λειτουργία","dBA","19","19"]
["Ψυκτικό μέσο","GWP","","","","675","675"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5"]
["","Αποχέτευση","","","","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC466A83","ARC466A83"]
["Στάνταρτ εξαρτήματα","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1"]
["","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m"]
["","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m"]
["","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Στάνταρτ εξαρτήματα","FTXTM40A2V1B","","","","","1"]