{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.032","0.037"]
["","Θέρμανση","","Ονομ.","kW","0.037","0.04"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","294","300"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","811","1040"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","272","295"]
["Βάρος","Μονάδα","","","kg","10","14.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","11.7","15.5"]
["","","","Μέτρια","m³/min","8","9.2"]
["","","","Χαμηλή","m³/min","6.3","5.7"]
["","","","Αθόρυβη λειτουργία","m³/min","5.2","4.6"]
["","","Θέρμανση","Υψ.","m³/min","12.2","17.7"]
["","","","Μέτρια","m³/min","7.5","11"]
["","","","Χαμηλή","m³/min","5.1","7.5"]
["","","","Αθόρυβη λειτουργία","m³/min","4.1","6.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","60","60"]
["","Θέρμανση","","","dBA","61","61"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","45","46"]
["","","","Μέτρια","dBA","33","32"]
["","","","Χαμηλή","dBA","25","24"]
["","","","Αθόρυβη λειτουργία","dBA","21","20"]
["","Θέρμανση","","Υψ.","dBA","45","46"]
["","","","Μέτρια","dBA","31","31"]
["","","","Χαμηλή","dBA","22","22"]
["","","","Αθόρυβη λειτουργία","dBA","19","19"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5"]
["","Αποχέτευση","","","","16 (εσωτερική διάμετρος εύκαμπτου σωλήνα σύνδεσης)","16 (εσωτερική διάμετρος εύκαμπτου σωλήνα σύνδεσης)"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC466A55","ARC466A55"]
["","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1"]
["","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]