{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30R2V1B / RXTM30A2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","0.70"]
["","Ονομ.","","kW","3.00"]
["","Μέγ.","","kW","4.50"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","0.80"]
["","Ονομ.","","kW","3.20"]
["","Μέγ.","","kW","6.70"]
["Ονομαστική απόδοση","EER","","","4.10"]
["","COP","","","5.34"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","366"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++"]
["","Απόδοση","Pdesign","kW","3.00"]
["","SEER","","","7.60"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","138"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A+++"]
["","Απόδοση","Pdesign","kW","3.00"]
["","SCOP/A","","","5.12"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","3.00"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","821"]