{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K / RXTP-N"]
[]
[]
[]
[]
["","","","","FTXTP25K3V1B / RXTP25N2V1B","FTXTP35K3V1B / RXTP35N2V1B"]
["Εξωτερική μονάδα","","","","RXTP25N2V1B","RXTP35N2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","0.70","0.70"]
["","Ονομ.","","kW","2.50","3.50"]
["","Μέγ.","","kW","4.00","4.40"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","0.80","0.80"]
["","Ονομ.","","kW","3.20","4.00"]
["","Μέγ.","","kW","6.20","6.70"]
["Ονομαστική απόδοση","EER","","","4.40","3.80"]
["","COP","","","4.95","4.44"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","285","460"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++"]
["","Απόδοση","Pdesign","kW","2.50","3.50"]
["","SEER","","","7.10","7.20"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","123","170"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++"]
["","Απόδοση","Pdesign","kW","2.50","3.00"]
["","SCOP/A","","","4.98","4.81"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","2.50","3.00"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","703","873"]
["Εύρος ενεργειακής αποδοτικότητας","","","","A+++ ~ D","A+++ ~ D"]