{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K / RXTP-N"]
[]
[]
[]
[]
["","","","","FTXTP35K3V1B / RXTP35N2V1B","FTXTP25K3V1B / RXTP25N2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","0.70","0.70"]
["","Μέγ.","","kW","4.40","4.00"]
["","Ονομ.","","kW","3.50","2.50"]
["Ονομαστική απόδοση","Ετήσια κατανάλωση ενέργειας","","kWh","460","285"]
["","EER","","","3.80","4.40"]
["","COP","","","4.44","4.95"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","4.00","3.20"]
["","Ελάχ.","","kW","0.80","0.80"]
["","Μέγ.","","kW","6.70","6.20"]
["Σημειώσεις","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","(2) - Ψύξη: T2: εσωτ. θερμ. 26,6°CDB, 19,4°CWB, εξωτ. θερμ. 48°CDB [Btu/hr/W]","(2) - Ψύξη: T2: εσωτ. θερμ. 26,6°CDB, 19,4°CWB, εξωτ. θερμ. 48°CDB [Btu/hr/W]"]
["","","","","(3) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(3) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]