{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","43"]
["","","","Μέτρια","dBA","35"]
["","","","Αθόρυβη λειτουργία","dBA","21"]
["","","","Χαμηλή","dBA","26"]
["","Ψύξη","","Μέτρια","dBA","35"]
["","","","Αθόρυβη λειτουργία","dBA","21"]
["","","","Χαμηλή","dBA","26"]
["","","","Υψ.","dBA","43"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1"]
["","Πλάκα στήριξης","","","","1"]
["","Αποσμητικό φίλτρο τιτανίου με επικάλυψη απατίτη","","","","2"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50"]
["","Συμπυκνωμάτων","","","","16 (εσωτερική διάμετρος εύκαμπτου σωλήνα σύνδεσης)"]
["Power input","Ψύξη","","Ονομ.","kW","0.030"]
["","Θέρμανση","","Ονομ.","kW","0.035"]
["Sound power level","Ψύξη","","","dBA","58"]
["","Θέρμανση","","","dBA","58"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","770"]
["","","","Βάθος","mm","225"]
["","","","Ύψος","mm","285"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["Βάρος","Μονάδα","","","kg","9.0"]
["Power supply","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Όνομα","","","","V1"]
["","Τάση","","","V","220-240"]
["Σημειώσεις","","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.03"]
["","Θέρμανση","","Ονομ.","kW","","0.035"]
["Περίβλημα","Χρώμα","","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","285"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","225"]
["Βάρος","Μονάδα","","","kg","","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","11.4"]
["","","","Μέτρια","m³/min","","8.2"]
["","","","Χαμηλή","m³/min","","5.4"]
["","","","Αθόρυβη λειτουργία","m³/min","","4.3"]
["","","Θέρμανση","Υψ.","m³/min","","10.8"]
["","","","Μέτρια","m³/min","","7.8"]
["","","","Χαμηλή","m³/min","","5.8"]
["","","","Αθόρυβη λειτουργία","m³/min","","4.9"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","58"]
["","Θέρμανση","","","dBA","","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","43"]
["","","","Μέτρια","dBA","","35"]
["","","","Χαμηλή","dBA","","26"]
["","","","Αθόρυβη λειτουργία","dBA","","21"]
["","Θέρμανση","","Υψ.","dBA","","43"]
["","","","Μέτρια","dBA","","35"]
["","","","Χαμηλή","dBA","","26"]
["","","","Αθόρυβη λειτουργία","dBA","","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","9.5"]
["","Αποχέτευση","","","","","16 (εσωτερική διάμετρος εύκαμπτου σωλήνα σύνδεσης)"]
["Χειριστήρια","Infrared remote control","","","","","ARC480A11"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","V1"]
["","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-240"]