{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-N"]
[]
[]
[]
[]
["","","","","","FTXTP25N5V1B","FTXTP35N5V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.032","0.032"]
["","Θέρμανση","","Ονομ.","kW","0.032","0.032"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","286","286"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","225","225"]
["Βάρος","Μονάδα","","","kg","9","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","11","11"]
["","","","Μέτρια","m³/min","7.9","7.9"]
["","","","Χαμηλή","m³/min","5","5"]
["","","","Αθόρυβη λειτουργία","m³/min","3.7","3.7"]
["","","Θέρμανση","Υψ.","m³/min","10.5","10.5"]
["","","","Μέτρια","m³/min","9","9"]
["","","","Χαμηλή","m³/min","5.5","5.5"]
["","","","Αθόρυβη λειτουργία","m³/min","4.4","4.4"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","58","58"]
["","Θέρμανση","","","dBA","58","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","43","43"]
["","","","Μέτρια","dBA","35","35"]
["","","","Χαμηλή","dBA","26","26"]
["","","","Αθόρυβη λειτουργία","dBA","21","21"]
["","Θέρμανση","","Υψ.","dBA","43","43"]
["","","","Μέτρια","dBA","35","35"]
["","","","Χαμηλή","dBA","26","26"]
["","","","Αθόρυβη λειτουργία","dBA","21","21"]
["Ψυκτικό μέσο","GWP","","","","675","675"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5"]
["","Αποχέτευση","","","","18","18"]
["Χειριστήρια","Infrared remote control","","","","ARC480A53","ARC480A53"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]