{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","43","50","51","53"]
["","","Ονομ.","dBA","41","47","48","51"]
["","","Χαμηλή","dBA","38","44","46","48"]
["","Ψύξη","Χαμηλή","dBA","38","44","46","48"]
["","","Υψ.","dBA","43","50","51","53"]
["","","Ονομ.","dBA","41","47","48","51"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","Εγχειρίδιο χειρισμού","Εγχειρίδιο χειρισμού","Εγχειρίδιο χειρισμού","Εγχειρίδιο χειρισμού"]
["","Εγχειρίδιο εγκατάστασης","","","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης"]
["","Στήριγμα για την εγκατάσταση","","","Στήριγμα για την εγκατάσταση","Στήριγμα για την εγκατάσταση","Στήριγμα για την εγκατάσταση","Στήριγμα για την εγκατάσταση"]
["","Προστατευτικό λάστιχο οπής","","","Προστατευτικό λάστιχο οπής","Προστατευτικό λάστιχο οπής","Προστατευτικό λάστιχο οπής","Προστατευτικό λάστιχο οπής"]
["","Δακτύλιος","","","Δακτύλιος","Δακτύλιος","Δακτύλιος","Δακτύλιος"]
["","Μόνωση συνδέσμου","","","Μόνωση συνδέσμου","Μόνωση συνδέσμου","Μόνωση συνδέσμου","Μόνωση συνδέσμου"]
["","Κάλυμμα","","","Κάλυμμα","Κάλυμμα","Κάλυμμα","Κάλυμμα"]
["","Σφιγκτήρες","","","Σφιγκτήρες","Σφιγκτήρες","Σφιγκτήρες","Σφιγκτήρες"]
["","Κοχλίες","","","Κοχλίες","Κοχλίες","Κοχλίες","Κοχλίες"]
["","Σχέδιο εγκατάστασης","","","Σχέδιο εγκατάστασης","Σχέδιο εγκατάστασης","Σχέδιο εγκατάστασης","Σχέδιο εγκατάστασης"]
["","Υλικό ανθεκτικό στη δημιουργία συμπυκνωμάτων","","","Υλικό ανθεκτικό στη δημιουργία συμπυκνωμάτων","Υλικό ανθεκτικό στη δημιουργία συμπυκνωμάτων","Υλικό ανθεκτικό στη δημιουργία συμπυκνωμάτων","Υλικό ανθεκτικό στη δημιουργία συμπυκνωμάτων"]
["","Καλωδίωση τηλεχειριστηρίου","","","Καλωδίωση τηλεχειριστηρίου","Καλωδίωση τηλεχειριστηρίου","Καλωδίωση τηλεχειριστηρίου","Καλωδίωση τηλεχειριστηρίου"]
["Χειριστήρια","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","9.52","9.52"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","15.9","15.9","15.9","15.9"]
["","Συμπυκνωμάτων","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Απορροφ. ισχύς","Ψύξη","Ονομ.","kW","0.117","0.238","0.238","0.276"]
["","Θέρμανση","Ονομ.","kW","0.117","0.238","0.238","0.276"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","55","62","63","65"]
["","Θέρμανση","","dBA","55","62","63","65"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","600","600","600","600"]
["","","Βάθος","mm","270","350","350","350"]
["","","Ύψος","mm","1,850","1,850","1,850","1,850"]
["Περίβλημα","Colour","","","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')"]
["Βάρος","Μονάδα","","kg","39","47","47","47"]
["Power supply","Φάση","","","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50/60","50/60","50/60","50/60"]
["","Τάση","","V","220-240/220","220-240/220","220-240/220","220-240/220"]