{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Εξωτερική μονάδα","","","","RXLG25M","RXLG35M"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.2","1.4"]
["","Ονομ.","","kW","2.5","3.5"]
["","Μέγ.","","kW","5.1","5.6"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.0","1.1"]
["","Ονομ.","","kW","4.5","5.6"]
["","Μέγ.","","kW","6.5, 3.5","7.0, 4.0"]
["Ονομαστική απόδοση","EER","","","3.52","3.43"]
["","COP","","","3.88","3.61"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","355","510"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Συνδέσεις σωληνώσεων","Συμπυκνωμάτων","Εξ.Διάμ.","χιλ.","18","18"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","χιλ.","9.5","9.5"]
["","Υγρό","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","6.35"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++","A++"]
["","Απόδοση","Pdesign","kW","2.50","3.50"]
["","SEER","","","6.99","6.59"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","131","186"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A+","A+"]
["","Απόδοση","Pdesign","kW","3.00","3.40"]
["","SCOP/A","","","4.25","4.01"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","988","1187"]
["Σημειώσεις","","","","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ","(1) - EER/COP σύμφωνα με το Eurovent 2012, για χρήση μόνο εκτός ΕΕ"]
["","","","","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°","(2) - Ονομαστική απόδοση: ψύξη σε ον. φορτίο 35°/27°, θέρμανση σε ον. φορτίο 7°/20°"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Για ονομ. ελ. απόδοση θέρμ. θέστε τον ανεμ. μονάδας σε SL tap","(6) - Για ονομ. ελ. απόδοση θέρμ. θέστε τον ανεμ. μονάδας σε SL tap"]
["","","","","(7) - Μέγιστη θερμαντική απόδοση σε εξωτερική θερμοκρασία -15°C","(7) - Μέγιστη θερμαντική απόδοση σε εξωτερική θερμοκρασία -15°C"]