{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.02"]
["","Θέρμανση","","Ονομ.","kW","0.03"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","600"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","750"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","238"]
["Βάρος","Μονάδα","","","kg","17"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9"]
["","","","Μέτρια","m³/min","6.7"]
["","","","Χαμηλή","m³/min","4.8"]
["","","","Αθόρυβη λειτουργία","m³/min","4"]
["","","Θέρμανση","Υψ.","m³/min","9.4"]
["","","","Μέτρια","m³/min","6.8"]
["","","","Χαμηλή","m³/min","5.3"]
["","","","Αθόρυβη λειτουργία","m³/min","4"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","53"]
["","Θέρμανση","","","dBA","53"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39"]
["","","","Μέτρια","dBA","32"]
["","","","Χαμηλή","dBA","25"]
["","","","Αθόρυβη λειτουργία","dBA","20"]
["","Θέρμανση","","Υψ.","dBA","39"]
["","","","Μέτρια","dBA","32"]
["","","","Χαμηλή","dBA","25"]
["","","","Αθόρυβη λειτουργία","dBA","19"]
["Ψυκτικό μέσο","GWP","","","","675"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5"]
["","Αποχέτευση","","","","VP20 (I.D. 20/O.D. 26)"]
["Χειριστήρια","Infrared remote control","","","","ARC466A66"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]