{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B / RXTM-A"]
[]
[]
[]
[]
["","","","","FVXTM30B2V1B / RXTM30A2V1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.2"]
["","Ονομ.","","kW","3"]
["","Μέγ.","","kW","4.4"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.2"]
["","Ονομ.","","kW","3.2"]
["","Μέγ.","","kW","6.2"]
["Ονομαστική απόδοση","EER","","","4.35"]
["","COP","","","4.45"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","345"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++"]
["","Απόδοση","Pdesign","kW","3"]
["","SEER","","","7.5"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","140"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A++"]
["","Απόδοση","Pdesign","kW","3"]
["","SCOP/A","","","4.75"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","3"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","884"]
["Σημειώσεις","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","(2) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","(3) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","(4) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]