{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":12,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","","","","","","48.0"]
["","","","Σε χαμηλή ταχύτητα ανεμιστήρα","dBA","","","","","","45.0"]
["","","","Σε μεσαία ταχύτητα ανεμιστήρα","dBA","","","","","","46.5"]
["","Ψύξη","","Σε χαμηλή ταχύτητα ανεμιστήρα","dBA","","","","","","45.0"]
["","","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","","","","","","48.0"]
["","","","Σε μεσαία ταχύτητα ανεμιστήρα","dBA","","","","","","46.5"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης και χειρισμού","","","","","","","","","1"]
["","Υλικό σφικτήρα καλωδίου","","","","","","","","","1"]
["","Ροδέλα γκρόβερ","","","","","","","","","2"]
["","Βίδα εξάγωνης κεφαλής","","","","","","","","","2"]
["","Απλή ροδέλα","","","","","","","","","8"]
["","Βίδα εξάγωνης κεφαλής με ροδέλα","","","","","","","","","49"]
["","Σωλήνα σύνδεσης αερίου","","","","","","","","","1"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","","","","","","1"]
["Ψυκτικό μέσο","GWP","","","","","","","","","675"]
["","Τύπος","","","","","","","","","R-32"]
["Ισχύς εισόδου - 50Hz","Ψύξη","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","","","","","","0.54"]
["","Θέρμανση","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","","","","","","0.54"]
["Απόδοση ψύξης","Συνολική απόδοση","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","","","","","","22.4"]
["","Ονομ.","","","kW","","","","","","22.4"]
["Piping connections","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","","","","","9.5"]
["","","","Τύπος","","","","","","","Σύνδεση με εκχείλωση"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","","","","","19.1"]
["","","","Τύπος","","","","","","","Φλάντζα"]
["","Συμπυκνωμάτων","","","","","","","","","BSP1"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","","","","","","75.0"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","","","","","1,490"]
["","","","Βάθος","mm","","","","","","1,100"]
["","","","Ύψος","mm","","","","","","470"]
["Περίβλημα","Υλικό","","","","","","","","","Γαλβανισμένο χαλυβδοέλασμα"]
["","Colour","","","","","","","","","Άβαφο"]
["Βάρος","Μονάδα","","","kg","","","","","","105"]
["Ανεμιστήρας","Εξωτερική στατική πίεση - 50Hz","","Υψ.","Pa","","","","","","250"]
["","","","Χαμηλή","Pa","","","","","","50"]
["","Εξωτερική στατική πίεση - 60Hz","","Υψ.","Pa","","","","","","250"]
["","","","Χαμηλή","Pa","","","","","","50"]
["","Ταχύτητα ροής αέρα  -50Hz","Ψύξη","Σε υψηλή ταχύτητα ανεμιστήρα","m³/min","","","","","","62"]
["","","","Σε χαμηλή ταχύτητα ανεμιστήρα","m³/min","","","","","","41"]
["Απόδοση θέρμανσης","Συνολική απόδοση","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","","","","","","25.0"]
["","Ονομ.","","","kW","","","","","","25.0"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","","","","","","6"]
["Power supply","Φάση","","","","","","","","","1~"]
["","Όνομα","","","","","","","","","VM"]
["","Συχνότητα","","","Hz","","","","","","50/60"]
["","Τάση","","","V","","","","","","220-240/220-230"]
["Απόδοση ψύξης","Συνολική απόδοση","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Απόδοση σε λειτουργία θέρμανσης","Συνολική απόδοση","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Ισχύς εισόδου - 50Hz","Ψύξη","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Θέρμανση","","Σε υψηλή ταχύτητα ανεμιστήρα","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","300","300","300","300","300","","470"]
["","","","Πλάτος","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Βάθος","mm","700","700","700","700","700","","1,100"]
["Βάρος","Μονάδα","","","kg","35","35","35","46","46","","115"]
["Περίβλημα","Χρώμα","","","","Άβαφο","Άβαφο","Άβαφο","Άβαφο","Άβαφο","","Άβαφο"]
["","Υλικό","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","","Γαλβανισμένο χαλυβδοέλασμα"]
["Απαιτούμενο διάκενο ψευδοροφής >-=-mm","mm","","","","350","350","350","350","350"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα - 50Hz","Ψύξη","Σε υψηλή ταχύτητα ανεμιστήρα","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","Σε χαμηλή ταχύτητα ανεμιστήρα","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","Εξωτερική στατική πίεση - 50Hz","","Υψ.","Pa","200","200","200","200","200","","250"]
["","Εξωτερική στατική πίεση - 60Hz","","Υψ.","Pa","200","200","200","200","200","","250"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","GWP","","","","675","675","675","675","675","","675"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","Σε μεσαία ταχύτητα ανεμιστήρα","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Σε χαμηλή ταχύτητα ανεμιστήρα","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Θέρμανση","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","Σε μεσαία ταχύτητα ανεμιστήρα","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Σε χαμηλή ταχύτητα ανεμιστήρα","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Συνδέσεις σωληνώσεων","Υγρό","","Τύπος","","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","","Σύνδεση με εκχείλωση"]
["","","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Αέριο","","Τύπος","","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","","Φλάντζα"]
["","","","ΕΞ.ΔΙΑΜ.","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Αποχέτευση","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Φίλτρο αέρα","Τύπος","","","","Πλέγμα ρητίνης","Πλέγμα ρητίνης","Πλέγμα ρητίνης","Πλέγμα ρητίνης","Πλέγμα ρητίνης"]
["Στάνταρτ εξαρτήματα","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Τροφοδοσία ισχύος","Όνομα","","","","VE","VE","VE","VE","VE","","VM"]
["","Φάση","","","","1~","1~","1~","1~","1~","","1~"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["","Τάση","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","6","6","6","6","6","","6"]
["Ανεμιστήρας","Εξωτερική στατική πίεση - 50Hz","","Χαμηλή","Pa","","","","","","","50"]
["","Εξωτερική στατική πίεση - 60Hz","","Χαμηλή","Pa","","","","","","","50"]
["Στάνταρτ εξαρτήματα","General safety precautions","","","","","","","","","","1"]
["","Wire clamp material","","","","","","","","","","1"]
["","Spring washer","","","","","","","","","","2"]
["","Hexagon head screw","","","","","","","","","","2"]
["","Plain washer","","","","","","","","","","8"]
["","Hexagon head screw with washer","","","","","","","","","","49"]
["","Gas connection pipe","","","","","","","","","","1"]