{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXSN-A2"]
[]
[]
[]
[]
["","","","","FXSN50A2VEB","FXSN71A2VEB","FXSN112A2VEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","38.0","39.0","42.0"]
["","","Σε χαμηλή ταχύτητα ανεμιστήρα","dBA","32.0","33.0","38.0"]
["","","Σε μεσαία ταχύτητα ανεμιστήρα","dBA","35.0","36.0","40.0"]
["","Ψύξη","Σε χαμηλή ταχύτητα ανεμιστήρα","dBA","31.0","32.0","34.0"]
["","","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","36.0","37.0","40.0"]
["","","Σε μεσαία ταχύτητα ανεμιστήρα","dBA","33.0","34.0","38.0"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης και χειρισμού","","","1","1","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","1","1","1"]
["","Μεταλλικός σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","","","1","1","1"]
["","Ροδέλα για στήριγμα ανάρτησης","","","8","8","8"]
["","Κοχλίες","","","40","40","40"]
["","Μόνωση συνδέσμου","","","2","2","2"]
["","Στεγανοποιητικό παρέμβυσμα","","","5","5","5"]
["","Σφιγκτήρες","","","4","4","4"]
["Ψυκτικό μέσο","GWP","","","1.0","1.0","1.0"]
["","Τύπος","","","R-744","R-744","R-744"]
["Απόδοση ψύξης","Συνολική απόδοση","Σε υψηλή ταχύτητα ανεμιστήρα","kW","5.60","8.00","12.50"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52","9.52"]
["","","Τύπος","","Χαλκοκόλληση-χαλκοκόλληση","Χαλκοκόλληση-χαλκοκόλληση","Χαλκοκόλληση-χαλκοκόλληση"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","12.7","12.7","12.7"]
["","","Τύπος","","Χαλκοκόλληση-χαλκοκόλληση","Χαλκοκόλληση-χαλκοκόλληση","Χαλκοκόλληση-χαλκοκόλληση"]
["","Συμπυκνωμάτων","","","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm"]
["Sound power level","Ψύξη","Σε υψηλή ταχύτητα ανεμιστήρα","dBA","61","63","66"]
["Φίλτρο αέρα","Type","","","Πλέγμα ρητίνης","Πλέγμα ρητίνης","Πλέγμα ρητίνης"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","700","1,000","1,400"]
["","","Βάθος","mm","800","800","800"]
["","","Ύψος","mm","245","245","245"]
["Περίβλημα","Υλικό","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["","Χρώμα","","","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)"]
["Βάρος","Μονάδα","","kg","31.0","40.0","50.0"]
["Ύψος αντλίας συμπυκνωμάτων","mm","","","625","625","625"]
["Απόδοση θέρμανσης","Συνολική απόδοση","Σε υψηλή ταχύτητα ανεμιστήρα","kW","6.30","9.00","14.0"]
["Power supply","Φάση","","","1~","1~","1~"]
["","Συχνότητα","","Hz","50/60","50/60","50/60"]
["","Όνομα","","","VE","VE","VE"]
["","Τάση","","V","220-240/220","220-240/220","220-240/220"]
["Σημειώσεις","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["","","","","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης.","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης.","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης."]
["","","","","(3) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA","(3) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA","(3) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA"]
["","","","","(4) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%.","(4) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%.","(4) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%."]
["","","","","(5) - Χρησιμοποιήστε έναν ασφαλειοδιακόπτη αντί για ασφάλεια.","(5) - Χρησιμοποιήστε έναν ασφαλειοδιακόπτη αντί για ασφάλεια.","(5) - Χρησιμοποιήστε έναν ασφαλειοδιακόπτη αντί για ασφάλεια."]
["","","","","(6) - MCA/MFA,; MCA= 1,25 x FLA,; MFA=< 4 x FLA,; H επόμενη χαμηλ. στάνταρ τιμή ασφ., ελάχ. 16A.","(6) - MCA/MFA,; MCA= 1,25 x FLA,; MFA=< 4 x FLA,; H επόμενη χαμηλ. στάνταρ τιμή ασφ., ελάχ. 16A.","(6) - MCA/MFA,; MCA= 1,25 x FLA,; MFA=< 4 x FLA,; H επόμενη χαμηλ. στάνταρ τιμή ασφ., ελάχ. 16A."]
["","","","","(7) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(7) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(7) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]