{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHCCU0180CL3","JEHCCU0210CL3"]
["Βάρος","Μονάδα","","","kg","80","81"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","1,101","1,101"]
["","","","Βάθος","mm","444","444"]
["","","","Ύψος","mm","662","662"]
["Περίβλημα","Colour","","","","Ανοικτό γκρι","Ανοικτό γκρι"]
["Ανεμιστήρας","Type","","","","Αξονικός","Αξονικός"]
["Power supply","Phase","","","","3~","3~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","400","400"]
["Σημειώσεις","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Η στάθμη ηχητικής πίεσης μετράται σε 10m σε ανηχοϊκό θάλαμο","(2) - Η στάθμη ηχητικής πίεσης μετράται σε 10m σε ανηχοϊκό θάλαμο"]
["","","","","","(3) - Η λειτουργία του βασίζεται στα φθοριούχα αέρια του θερμοκηπίου","(3) - Η λειτουργία του βασίζεται στα φθοριούχα αέρια του θερμοκηπίου"]
["Ψυκτική απόδοση","Χαμηλή θερμοκρασία","R-448A","Ονομ.","kW","0.98"]
["","","R-449A","Ονομ.","kW","0.98"]
["Ισχύς εισόδου","Χαμηλή θερμοκρασία","R-448A","Ονομ.","kW","0.98"]
["","","R-449A","Ονομ.","kW","0.98"]
["COP","Χαμηλή θερμοκρασία","","R-448A","","1.00"]
["","","","R-449A","","1.00"]
["Παράμετροι σε πλήρες φορτίο και θερμ. περιβάλλοντος 32°C (Σημείο A)","R-448A","Te -10°C","Ονομαστική απόδοση ψύξης (ΡΑ)","kW","0.98"]
["","","","Ονομαστική ισχύς εισόδου (DA)","kW","0.98"]
["","","","Ονομαστικός COP (COPA)","","1.00"]
["","R-449A","Te -10°C","Ονομαστική απόδοση ψύξης (ΡΑ)","kW","0.98"]
["","","","Ονομαστική ισχύς εισόδου (DA)","kW","0.98"]
["","","","Ονομαστικός COP (COPA)","","1.00"]
["Παράμετροι σε πλήρες φορτίο και θερμ. περιβάλλοντος 25°C","R-448A","Te -35°C","Δηλωμένο COP (COP2)","","1.15"]
["","","","Ισχύς εισόδου (D2)","kW","1.00"]
["","R-449A","Te -35°C","Δηλωμένο COP (COP2)","","1.15"]
["Ψυκτικό μέσο","Τύπος 5","","","","R-448A"]
["","GWP Τύπος 5","","","","1,387"]