{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRLEQ-BY1"]
[]
[]
[]
[]
["","","","","","LRLEQ3BY1","LRLEQ4BY1"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","1","1"]
["Ψυκτική απόδοση","Χαμηλή θερμοκρασία","","kW","kW","2.78 (1)","3.62 (1)"]
["Βάρος","Μονάδα","","","kg","130","130"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","14.4","14.4"]
["","GWP","","","","2,087.5","2,087.5"]
["","Φορτίο","","","kg","6.90","6.90"]
["","Τύπος","","","","R-410A","R-410A"]
["Κινητ. ανεμ.","Έξοδος","","","W","70","70"]
["","Μετάδοση κίνησης","","","","Άμεσης οδήγησης","Άμεσης οδήγησης"]
["Εναλλάκτης θερμότητας","Τύπος","","","","Στοιχείο διασταυρούμενων πτερυγίων","Στοιχείο διασταυρούμενων πτερυγίων"]
["Ισχύς εισόδου","Χαμηλή θερμοκρασία","","Ονομ.","kW","2.60 (1)","3.41 (1)"]
["COP","Χαμηλή θερμοκρασία","","Ονομ.","","1.07 (1)","1.06 (1)"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","900","900"]
["","","","Βάθος","mm","320","320"]
["","","","Ύψος","mm","1,345","1,345"]
["Casing","Colour","","","","Λευκό Daikin","Λευκό Daikin"]
["Fan","Type","","","","Ελικοειδής","Ελικοειδής"]
["","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","106","106"]
["","Ποσότητα","","","","2","2"]
["Power supply","Phase","","","","3N~","3N~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","380-415","380-415"]
["Σημειώσεις","","","","","(1) - Ψύξη: θερμοκρασία εξάτμισης -35°C, εξωτερική θερμ. 32°C, είσοδος SH10°C","(1) - Ψύξη: θερμοκρασία εξάτμισης -35°C, εξωτερική θερμ. 32°C, είσοδος SH10°C"]
["","","","","","(2) - Δεδομένα ηχητικής πίεσης: μέτρηση 1m εμπρός από τη μονάδα, σε ύψος 1,5m","(2) - Δεδομένα ηχητικής πίεσης: μέτρηση 1m εμπρός από τη μονάδα, σε ύψος 1,5m"]