{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Στάνταρτ εξαρτήματα","Δήλωση συμμόρφωσης","","","","1"]
["Βάρος","Μονάδα","","","kg","173"]
["Ψυκτικό μέσο","GWP","","","","1.0"]
["","Charge","","","kg","3.20"]
["Κινητήρας ανεμιστήρα","Output","","","W","350"]
["Εναλλάκτης θερμότητας","Τύπος","","","","Στοιχείο διασταυρούμενων πτερυγίων"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","635"]
["","","","Βάθος","mm","765"]
["","","","Ύψος","mm","1,680"]
["Περίβλημα","Χρώμα","","","","Κρεμ_"]
["Ανεμιστήρας","Τύπος","","","","Ανεμιστήρας έλικας"]
["","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","102"]
["","Ποσότητα","","","","1"]
["Power supply","Φάση","","","","3N~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","380-415"]
["Σημειώσεις","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Συμπιεστής 1"]
["","","","","","(3) - Συμπιεστής 2"]
["","","","","","(4) - Συμπιεστής 3"]
["","","","","","(5) - Πλήρωση της μονάδας από το εργοστάσιο"]
["","","","","","(6) - Επιτρέπεται μόνο χρήση K65 με πίεση σχεδιασμού Επιτρέπεται χρήση 120 bar για συνδέσεις σωληνώσεων AC."]
["","","","","","(7) - Η πίεση βαλβίδας ασφαλείας επισημαίνεται ως πίεση μετρητή."]
["","","","","","(8) - Επιτρέπεται μόνο χρήση K65 με πίεση σχεδιασμού Επιτρέπεται χρήση 90 bar για τις σωληνώσεις ψύξης."]