{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC30YV"]
[]
[]
[]
[]
["","","","","","MC30YVM"]
["Τύπος","","","","","Ιονιστής"]
["Εφαρμογή","","","","","Τύπου δαπέδου"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Ύψος","χιλ.","450"]
["","","","Πλάτος","χιλ.","270"]
["","","","Βάθος","χιλ.","270"]
["Βάρος","Μονάδα","","","kg","5.8"]
["Κατάλληλο εμβαδόν δωματίου","m²","","","","23 (1), 46 (2)"]
["CADR","m³/ώρα","","","","180"]
["Λειτουργία φιλτραρίσματος αέρα","Ισχύς εισόδου","","Turbo","kW","0.025"]
["","","","M","kW","0.015"]
["","","","Αθόρυβο","kW","0.008"]
["Στάθμη ηχητικής πίεσης","Λειτουργία φιλτραρίσματος αέρα","","Turbo","dBA","37"]
["","","","Μέτρια","dBA","27"]
["","","","Αθόρυβο","dBA","19"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Λειτουργία φιλτραρίσματος αέρα","Turbo","m³/ώρα","180"]
["","","","Μέτρια","m³/ώρα","120"]
["","","","Αθόρυβο","m³/ώρα","60"]
["Μέθοδος συλλογής σκόνης","","","","","Ηλεκτροστατικό φίλτρο HEPA"]
["Deodorizing method","","","","","Flash streamer + Καταλύτης με αποσμητική δράση"]
["Στάνταρτ εξαρτήματα","Ηλεκτροστατικό φίλτρο HEPA","","","","1"]
["","Αποσμητικό φίλτρο","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","1"]
["Καλώδιο τροφοδοσίας","m","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Συχνότητα","","","Hz","50/60"]
["","Τάση","","","V","220-240/220-230"]
["Ρεύμα λειτουργίας","Λειτουργία φιλτραρίσματος αέρα","","Turbo","A","0.13"]
["","","","Μέτρια","A","0.09"]
["","","","Αθόρυβο","A","0.08"]
["Σημειώσεις","","","","","(1) - Το κατάλληλο εμβαδόν δωματίου αρμόζει για τη λειτουργία μονάδας σε μέγιστη ταχύτητα ανεμιστήρα (HH). Ο χώρος δωματίου εφαρμογής υποδεικνύει το χώρο όπου συγκεκριμένη ποσότητα σωματιδίων σκόνης μπορεί να απομακρυνθεί μέσα σε 30 λεπτά. (JEM 1467)"]
["","","","","","(2) - Το κατάλληλο εμβαδόν δωματίου αρμόζει για τη λειτουργία μονάδας σε μέγιστη ταχύτητα ανεμιστήρα (HH). Το κατάλληλο εμβαδόν δωματίου υπολογίστηκε σύμφωνα με το πρότυπο NRCC-54013 με τη χρήση CADR καπνίσματος τσιγάρου που ελέγχθηκε σύμφωνα με το JEM1467."]
["","","","","","(3) - Μετατροπή στα πρότυπα CADR από τιμές δοκιμών σε συμφωνία με το JEM1467."]
["","","","","","(4) - Τα επίπεδα ήχου λειτουργίας είναι οι μέσες τιμές που μετρούνται σε απόσταση 1 μ. από το εμπρόσθιο, αριστερό, δεξιό και άνω μέρος της μονάδας. (Αυτά ισοδυναμούν με τις τιμές σε ανηχοϊκό θάλαμο)"]
["","","","","","(5) - Στη μονάδα είναι προσαρτημένο ηλεκτροστατικό φίλτρο HEPA."]
["","","","","","(6) - Άλλη λειτουργία: Λειτουργία αυτόματης επανεκκίνησης."]