{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Τύπος","","","","","Ιονιστής με λειτουργία ύγρανσης"]
["Εφαρμογή","","","","","Τύπου δαπέδου"]
["Περίβλημα","Χρώμα","","","","Λευκό (N9. 0)"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","600 (5)"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","395"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","287"]
["Βάρος","Μονάδα","","","kg","12.5"]
["Κατάλληλο εμβαδόν δωματίου","m²","","","","48 (1), 96 (2)"]
["CADR","m³/ώρα","","","","375"]
["Λειτουργία φιλτραρίσματος αέρα","Ισχύς εισόδου","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","ΧΑΜ.","kW","0.01"]
["","","","Αθόρυβο","kW","0.008"]
["Λειτουργία ύγρανσης","Ισχύς εισόδου","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","ΧΑΜ.","kW","0.012"]
["","","","Αθόρυβο","kW","0.011"]
["","Χωρητικότητα δεξαμενής νερού","","","l","3.6"]
["Στάθμη ηχητικής πίεσης","Λειτουργία φιλτραρίσματος αέρα","","Turbo","dBA","54"]
["","","","Μέτρια","dBA","37"]
["","","","Χαμηλή","dBA","27"]
["","","","Αθόρυβο","dBA","18"]
["","Λειτουργία ύγρανσης","","Turbo","dBA","54"]
["","","","Μέτρια","dBA","37"]
["","","","Χαμηλή","dBA","27"]
["","","","Αθόρυβο","dBA","23"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Λειτουργία φιλτραρίσματος αέρα","Turbo","m³/ώρα","420"]
["","","","Μέτρια","m³/ώρα","210"]
["","","","Χαμηλή","m³/ώρα","132"]
["","","","Αθόρυβο","m³/ώρα","60"]
["","","Λειτουργία ύγρανσης","Turbo","m³/ώρα","420"]
["","","","Μέτρια","m³/ώρα","210"]
["","","","Χαμηλή","m³/ώρα","132"]
["","","","Αθόρυβο","m³/ώρα","102"]
["Μέθοδος συλλογής σκόνης","","","","","Ηλεκτροστατικό φίλτρο HEPA"]
["Μέθοδος απόσμησης","","","","","Flash streamer + Καταλύτης με αποσμητική δράση"]
["Στάνταρτ εξαρτήματα","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Καλώδιο τροφοδοσίας","m","","","","2"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50/60"]
["","Τάση","","","V","220-240/220-230"]
["Σημειώσεις","","","","","(1) - Ο τομέας κάλυψης αρμόζει για τη λειτουργία μονάδας σε μέγιστη ταχύτητα ανεμιστήρα (HH). Ο τομέας κάλυψης υποδεικνύει το χώρο όπου συγκεκριμένη ποσότητα σωματιδίων σκόνης μπορεί να απομακρυνθεί μέσα σε 30 λεπτά."]
["","","","","","(2) - Μετατροπή στα πρότυπα NRCC από τιμές δοκιμών σε συμφωνία με το JEM1467."]
["","","","","","(3) - Τα επίπεδα ήχου λειτουργίας είναι οι μέσες τιμές που μετρούνται σε απόσταση 1 μ. από το εμπρόσθιο, αριστερό, δεξιό και άνω μέρος της μονάδας. (Αυτά ισοδυναμούν με τις τιμές σε ανηχοϊκό θάλαμο)"]