{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":5,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RDXYQ-TA"]
[]
[]
[]
[]
["","","","","RDXYQ5TAV1B"]
["Στάθμη ηχητικής πίεσης","Ψύξη","Ονομ.","dBA","54 (5)"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης και χειρισμού","","","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","1"]
["","Κοχλίες","","","1"]
["","Πλαστικός σφιγκτήρας","","","1"]
["","Ταινία εύκαμπτου σωλήνα","","","1"]
["Βάρος","Μονάδα","","kg","103"]
["Ψυκτικό μέσο","Τύπος","","","R-410A"]
["Συνδέσεις σωληνώσεων","Συμπυκνωμάτων","Εξ.Διάμ.","mm","32"]
["Sound power level","Ψύξη","Ονομ.","dBA","81 (4)"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","1,456"]
["","","Βάθος","mm","1,044"]
["","","Ύψος","mm","397"]
["","Αγωγός","Ύψος","mm","298"]
["","","Πλάτος","mm","1,196"]
["Power supply","Φάση","","","1N~"]
["","Συχνότητα","","Hz","50"]
["","Όνομα","","","V1"]
["","Τάση","","V","220-240"]
["Σημειώσεις","","","","(1) - Οι ονομ. αποδόσεις ψύξης βασίζονται σε: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδ. σωλ. ψυκτικού: 5m, υψομετρική διαφορά: 0m. Δεδ. για στάνταρ σειρές απόδ."]
["","","","","(2) - Οι ονομ. αποδ. θέρμ. βασίζονται στα εξής: εσ. θερμοκρ.: 20°CDB, εξ. θερμοκρ.: 7°CDB, 6°CWB,  ισοδ. σωλ. ψυκτικού: 5m, υψομετρική διαφορά: 0m. Δεδ. για στάνταρ σειρές απόδ."]
["","","","","(3) - Ο πραγμ. αρ. μονάδων εξαρτάται από τον τύπο εσωτ. μονάδας (VRV DX εσωτ. κλπ.) και τον περιορισμό λόγου σύνδ. για το σύστημα (ήτοι:; 50% ≤ CR ≤ 130%)."]
["","","","","(4) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["","","","","(5) - Η στάθμη ηχητικής πίεσης είναι μία σχετική τιμή που εξαρτάται από την απόσταση και το ακουστικό περιβάλλον. Για περισσότερες λεπτομέρειες, ανατρέξτε στο εγχειρίδιο οδηγιών. Ονομαστική ταχύτητα ροής αέρα, ESP 60 Pa."]
["","","","","(6) - Ανατρέξτε στην επιλογή σωλήνων ψυκτικού μέσου ή στο εγχειρίδιο εγκατάστασης"]
["","","","","(7) - Σύμφωνα με το EN/IEC 61000-3-12, ενδέχεται να είναι απαραίτητη η συνεννόηση με τον υπεύθυνο του δικτύου διανομής για να βεβαιωθείτε ότι ο εξοπλισμός συνδέεται μόνο σε παροχή με Ssc  ≥ ελάχιστης τιμής Ssc"]
["","","","","(8) - Οι τιμές θορύβου μετρώνται σε ημιανηχοϊκό θάλαμο."]
["","","","","(9) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]