{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B5V1B","RXA42B2V1B","RXA50B2V1B","RXA50B5V1B"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","734","734","734"]
["","","","Πλάτος","mm","","870","870","954"]
["","","","Βάθος","mm","","373","373","401"]
["Βάρος","Μονάδα","","","kg","","50","50","49"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","-10","-10","-10"]
["","","","Μέγ.","°CDB","","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","-15","-15","-15"]
["","","","Μέγ.","°CWB","","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","","48.0","48.0","48"]
["","Θέρμανση","","Ονομ.","dBA","","48.0","48.0","48"]
["Ψυκτικό μέσο","Τύπος","","","","","R-32","R-32","R-32"]
["","Φορτίο","","","kg","","1.10","1.10","1.1"]
["","Φορτίο","","","tCO2Eq","","0.75","0.75","0.75"]
["","GWP","","","","","675","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","30","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","20","20","20"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","1","1","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","","1","1","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","","1","1","1"]
["","Πώμα εξόδου συμπυκνωμάτων","","","","","3","3","3"]
["","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","1","1","1"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50"]
["","Τάση","","","V","","220-240","220-240","220-240"]
["Σημειώσεις","","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]