{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","","","30.1","30.6","48.9"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","","","25.6","27.2","43.1"]
["","","","Εξαιρετικά χαμηλές","cfm","","","1063","1080","1727"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","","904","960","1522"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","550","550","550","550","735"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","765","765","765","765","825"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","285","285","285","285","300"]
["Βάρος","Μονάδα","","","kg","34","34","34","39","47"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","780","780","780","790","670"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","740","740","740","780","670"]
["Συμπιεστής","Type","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10","-10","-10","-10"]
["","","","Μέγ.","°CDB","46","46","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-25","-25","-25","-25","-25"]
["","","","Μέγ.","°CWB","18","18","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","46","48","48","48"]
["","Θέρμανση","","Υψ.","dBA","47","47","48","48","48"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Φορτίο","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Φορτίο","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20","20","20","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15","15","15","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]