{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":14,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-M"]
[]
[]
[]
[]
["","","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B","RXP50M2V1B","RXP50M5V1B","RXP60M2V1B","RXP60M5V1B","RXP71M2V1B","RXP71M5V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","550","550","550","734","734","734","734","734","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","658","658","658","870","870","870","870","870","870"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","275","275","275","373","373","373","373","373","373"]
["Βάρος","Μονάδα","","","kg","26","26","28","46.0","46.0","50.0","50.0","50.0","50.0"]
["Συμπιεστής","Type","","","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Μέγ.","°CDB","48","48","48","46","48","46","48","46","48"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46","46","48","47","47","49","49","52","52"]
["","Θέρμανση","","Ονομ.","dBA","47","47","48","49","49","49","49","52","52"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Φορτίο","","","kg","0.55","0.55","0.70","0.90","0.90","1.15","1.15","1.15","1.15"]
["","Φορτίο","","","tCO2Eq","0.37","0.37","0.48","0.61","0.61","0.78","0.78","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675","675","675","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","15","15","15","30","30","30","30","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","12","12","12","20","20","20","20","20","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1"]
["","Drain cap","","","","","","","3","3","3","3","3","3"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Στάνταρτ εξαρτήματα","General safety precautions","","","","1","1","1"]