{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","47","","47","","48","48","48"]
["","Ψύξη","","Υψ.","dBA","46","","46","","48","48","48"]
["Στάνταρτ εξαρτήματα","Σύνδεσμος (έξοδος συμπυκνωμάτων)","","","","1","","1"]
["","Εγχειρίδιο εγκατάστασης","","","","1","","1","","1","1","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Φορτίο","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Τύπος","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","σ.α.λ.","780","","780","","780","790","670"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","σ.α.λ.","740","","740","","740","780","670"]
["Piping connections","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","","15","","15","15","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Συμπιεστής","Type","","","","Ερμητικά κλειστός συμπιεστής swing","","Ερμητικά κλειστός συμπιεστής swing","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","765","","765","","765","765","825"]
["","","","Βάθος","mm","285","","285","","285","285","300"]
["","","","Ύψος","mm","550","","550","","550","550","735"]
["Βάρος","Μονάδα","","","kg","34","","34","","34","39","47"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","","","","904","960","1,522"]
["","","Ψύξη","Εξαιρετικά χαμηλές","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","","1~","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","","50","","50","50","50"]
["","Τάση","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα","","(4) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα","","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","","(5) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","550","","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","765","","765"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","285","","285"]
["Βάρος","Μονάδα","","","kg","","34","","34"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","","780","","780"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","","740","","740"]
["Συμπιεστής","Type","","","","","Ερμητικά κλειστός συμπιεστής swing","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","-10","","-10"]
["","","","Μέγ.","°CDB","","46","","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","-15","","-15"]
["","","","Μέγ.","°CWB","","18","","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","46","","46"]
["","Θέρμανση","","Υψ.","dBA","","47","","47"]
["Ψυκτικό μέσο","Τύπος","","","","","R-410A","","R-410A"]
["","Φορτίο","","","kg","","1.0","","1.0"]
["","Φορτίο","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","20","","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","15","","15"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~","","1~"]
["","Συχνότητα","","","Hz","","50","","50"]
["","Τάση","","","V","","220-240","","220-240"]
["Στάνταρτ εξαρτήματα","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","","","","1","1","1"]