{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","47","47","48","48"]
["","Ψύξη","","Υψ.","dBA","46","46","48","48"]
["Στάνταρτ εξαρτήματα","Πώμα εξόδου συμπυκνωμάτων","","","","1","1","","1"]
["","Εγχειρίδιο εγκατάστασης","","","","1","1","1","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","1","1","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","1","1","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Φορτίο","","","kg","1.0","1.0","1.20","1.3"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","rpm","780","780","780","790"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","rpm","740","740","740","780"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","46","46","46","46"]
["","","","Ελάχ.","°CDB","-10","-10","-10","-10"]
["","Θέρμανση","Περιβάλλον","Μέγ.","°CWB","18","18","18","18"]
["","","","Ελάχ.","°CWB","-15","-15","-15","-15"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","","0.020 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","765","765","765","765"]
["","","","Βάθος","χιλ.","285","285","285","285"]
["","","","Ύψος","χιλ.","550","550","550","550"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Βάρος","Μονάδα","","","kg","34","34","34","39"]
["Fan","Ταχύτητα ροής αέρα","Θέρμανση","Εξαιρετικά χαμηλές","cfm","904","904","904","960"]
["","","","Εξαιρετικά χαμηλές","m³/min","25.6","25.6","25.6","27.2"]
["","","Ψύξη","Εξαιρετικά χαμηλές","m³/min","30.1","30.1","30.1","30.6"]
["","","","Εξαιρετικά χαμηλές","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(4) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Στάνταρτ εξαρτήματα","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","","1"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","","","","","48.9","45.0"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","","","","","43.1","46.3"]
["","","","Εξαιρετικά χαμηλές","cfm","","","","","1727","1589"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","","","","1522","1635"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","","","","","735","735"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","","","","","825","825"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","","","","","300","300"]
["Βάρος","Μονάδα","","","kg","","","","","47","48"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","","","","","670"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","","","","","670"]
["Συμπιεστής","Τύπος","","","","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","","","","-10","-10"]
["","","","Μέγ.","°CDB","","","","","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","","","","-15","-15"]
["","","","Μέγ.","°CWB","","","","","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","","48","49"]
["","","","Χαμηλή","dBA","","","","","44","46"]
["","Θέρμανση","","Υψ.","dBA","","","","","48","49"]
["","","","Χαμηλή","dBA","","","","","45","46"]
["Ψυκτικό μέσο","Τύπος","","","","","","","","R-410A","R-410A"]
["","Φορτίο","","","kg","","","","","1.7","1.5"]
["","Φορτίο","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","","","","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","","","","0.020 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0.020 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","","","","20.0","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","","","","1~","1~"]
["","Συχνότητα","","","Hz","","","","","50","50"]
["","Τάση","","","V","","","","","220-230-240","220-230-240"]
["Σημειώσεις","","","","","","","","","","(1) - 230V"]