{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","734","734","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","870","870","870"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","373","373","373"]
["Βάρος","Μονάδα","","","kg","52","52","52"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","62.0","63.0","64.0"]
["","Θέρμανση","","","dBA","62.0","63.0","64.0"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","48.0","49.0","50.0"]
["","Θέρμανση","","Ονομ.","dBA","48.0","49.0","50.0"]
["Ψυκτικό μέσο","Τύπος","","","","","R-32"]
["","Φορτίο","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675.0","675.0","675.0"]
["","Φορτίο","","","tCO2Eq","1.05","1.05","1.05"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.50","12.7","12.7"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","50","50","50"]
["","","Σύστημα","Χωρίς φορτίο","m","30","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30.0","30.0","30.0"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","","220-240"]