{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","734","734","734"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","870","870","870"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","373","373","373"]
["Βάρος","Μονάδα","","","kg","52","52","52"]
["Compressor","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-20","-20","-20"]
["","","","Μέγ.","°CDB","52","52","52"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-21","-21","-21"]
["","","","Μέγ.","°CWB","18","18","18"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","62","63","64"]
["","Θέρμανση","","","dBA","62","63","64"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","48","49","50"]
["","Θέρμανση","","Ονομ.","dBA","48","49","50"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32"]
["","Φορτίο","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Φορτίο","","","tCO2Eq","1.05","1.05","1.05"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","χιλ.","9.52","12.7","12.7"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","50","50","50"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30","30","30"]
["Στάνταρτ εξαρτήματα","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Στάνταρτ εξαρτήματα","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]