{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","1,680"]
["","","","Πλάτος","mm","930"]
["","","","Βάθος","mm","765"]
["Βάρος","Μονάδα","","","kg","183.0"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός, σπειροειδής συμπιεστής"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-5.0"]
["","","","Μέγ.","°CDB","46.0"]
["","Θέρμανση","Περιβάλλον","Ελάχ.","°CWB","-15.0"]
["","","","Μέγ.","°CWB","15.0"]
["Sound power level","Ψύξη","","","dBA","78.0"]
["","Θέρμανση","","","dBA","78.0"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A"]
["","Φορτίο","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","22.2"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","100"]
["","","Σύστημα","Χωρίς φορτίο","m","30"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1"]
["","Σωλήνες σύνδεσης","","","","4"]
["Power supply","Φάση","","","","3N~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","380-415"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","25"]
["Σημειώσεις","","","","","(1) - Η τροφοδοσία ρεύματος προς της εσωτερική μονάδα FDQ είναι ξεχωριστή."]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","1680"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","930"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","765"]
["Βάρος","Μονάδα","","","kg","","184.0"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός, σπειροειδής συμπιεστής"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","-5.0"]
["","","","Μέγ.","°CDB","","46.0"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","-15.0"]
["","","","Μέγ.","°CWB","","15.0"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","78.0"]
["","Θέρμανση","","","dBA","","78.0"]
["Ψυκτικό μέσο","Φορτίο","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Φορτίο","","","tCO2Eq","","19.4"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","12.70"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","22.2"]
["","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","100"]
["","","Σύστημα","Χωρίς φορτίο","m","","30"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Τροφοδοσία ισχύος","Συχνότητα","","","Hz","","50"]
["Ρεύμα - 50Hz","Μέγιστα αμπέρ ασφάλειας (MFA)","","","A","","25"]