{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53C"]
[]
[]
[]
[]
["","","","","BRC1E53C7"]
["Συσκευασία","Υλικό","","","Κιβώτιο_"]
["","Βάρος","","kg","0.05"]
["Θερμοκρασία περιβάλλοντος","Σχετική υγρασία <","","%","95"]
["Διαστάσεις","Μονάδα με στεγανοποίηση","Πλάτος","mm","160"]
["","","Ύψος","mm","55"]
["","","Βάθος","mm","150"]
["","Μονάδα","Πλάτος","mm","120"]
["","","Βάθος","mm","19"]
["","","Ύψος","mm","120"]
["Περίβλημα","Κάλυμμα κουμπιών","","","όχι"]
["","Χρώμα","","","Fresh white ('κατάλευκο')"]
["","LED Λειτουργίας","Χρώμα","","Πράσινο"]
["LCD","Τύπος","","","Πλήρη εικονοστοιχεία (160 x 255)"]
["","Οπίσθια λυχνία","Χρώμα","","Λευκό"]
["","Διαστάσεις","Πλάτος","mm","68.85"]
["","","Ύψος","mm","43.2"]
["Βάρος","Μονάδα με στεγανοποίηση","","kg","0.415"]
["","Μονάδα","","kg","0.200"]
["Εφεδρεία για περίπτωση διακοπής ρεύματος","","","","Ναι (Το ρολόι θα συνεχίσει να λειτουργεί για μια περίοδο που δεν θα υπερβαίνει τις 48 ώρες)"]
["Συνδέσεις καλωδιώσεων","Μήκος καλωδίου","Μέγ.","m","500"]