{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H519K"]
[]
[]
[]
[]
["","","","","BRC1H519K."]
["Συσκευασία","Υλικό","","","Χαρτόνι"]
["","Βάρος","","kg","0.0850"]
["Θερμοκρασία περιβάλλοντος","Σχετική υγρασία <","","%","95"]
["Διαστάσεις","Μονάδα με στεγανοποίηση","Πλάτος","mm","217"]
["","","Ύψος","mm","50"]
["","","Βάθος","mm","161"]
["","Μονάδα","Πλάτος","mm","85"]
["","","Βάθος","mm","25"]
["","","Ύψος","mm","85"]
["Περίβλημα","Κάλυμμα κουμπιών","","","όχι"]
["","Χρώμα","","","Black"]
["","LED Λειτουργίας","Χρώμα","","Blue status indicator"]
["LCD","Τύπος","","","100 x 150 dots"]
["","Οπίσθια λυχνία","Χρώμα","","Λευκό"]
["","Διαστάσεις","Πλάτος","mm","28.0"]
["","","Ύψος","mm","40.7"]
["Βάρος","Μονάδα με στεγανοποίηση","","kg","0.317"]
["","Μονάδα","","kg","0.110"]
["Συνδέσεις καλωδιώσεων","Μήκος καλωδίου","Μέγ.","m","500"]