{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","EHYHBH05AAV3 / EVLQ05CAV3","EHYHBH08AAV3 / EVLQ08CAV3"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.80, 1.80","1.80, 1.80"]
["","Ονομ.","","kW","4.40, 4.03","7.40, 6.89"]
["","Μέγ.","","kW","5.12, 4.90","10.02, 9.53"]
["Ισχύς εισόδου","Θέρμανση","Ονομ.","kW","0.87, 1.13","1.66, 2.01"]
["COP","","","","5.04, 3.58","4.45, 3.42"]
["Εύρος ενεργειακής αποδοτικότητας","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Σημειώσεις","","","","(1) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Συνθήκη: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]