{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","37.0","37.0","31.0","31.0"]
["","","","Μέτρια","dBA","34.0","34.0","28.0","28.0"]
["","","","Χαμηλή","dBA","29.0","29.0","25.0","25.0"]
["","Ψύξη","","Medium","dBA","32.0","32.0","28.0","28.0"]
["","","","Χαμηλή","dBA","29.0","29.0","25.0","25.0"]
["","","","Υψ.","dBA","35.0","35.0","30.0","30.0"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","","1","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","","1","1","1","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","","1","1","1","1"]
["","Μεταλλικός σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","","","","1","1","1","1"]
["","Ροδέλα για στήριγμα ανάρτησης","","","","8","8","8","8"]
["","Κοχλίες","","","","40","40","40","40"]
["","Μόνωση συνδέσμου","","","","2","2","2","2"]
["","Φύλλα στεγανοποίησης","","","","5","5","5","5"]
["","Σφιγκτήρες","","","","4","4","4","4"]
["Control systems","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Συνδέσεις σωληνώσεων","Υγρού","","ΕΞ.ΔΙΑΜ.","χιλ.","6.35","6.35","6.35","9.52"]
["","Αερίου","","Εξ.Διάμ.","χιλ.","9.52","12.70","12.70","15.90"]
["","Συμπυκνωμάτων","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","60","60","56","56"]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","700","700","1,000","1,000"]
["","","","Βάθος","χιλ.","800","800","800","800"]
["","","","Ύψος","χιλ.","245","245","245","245"]
["Casing","Material","","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["","Χρώμα","","","","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)","Άβαφο (γαλβανισμένο)"]
["Βάρος","Μονάδα","","","kg","28.0","28.0","35.0","35.0"]
["Fan","Εξωτερική στατική πίεση","","Υψ.","Pa","150","150","150","150"]
["","","","Ονομ.","Pa","30","30","30","30"]
["","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","15.0","15.0","18.0","18.0"]
["","","","Χαμηλή","m³/min","10.5","10.5","12.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0","15.0"]
["","","Ψύξη","Χαμηλή","m³/min","10.5","10.5","12.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0","15.0"]
["","","","Υψ.","m³/min","15.0","15.0","18.0","18.0"]
["Ύψος αντλίας συμπυκνωμάτων","χιλ.","","","","625","625","625","625"]
["Power supply","Φάση","","","","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50/60","50/60","50/60","50/60"]
["","Τάση","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Σημειώσεις","","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]