{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW"]
[]
[]
[]
[]
["","","","","","FTXG20LV1BW"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.023, 0.023, 0.023"]
["","Θέρμανση","","Ονομ.","kW","0.031, 0.031, 0.031"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","303"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","998"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","212"]
["Βάρος","Μονάδα","","","kg","12.0"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","8.9"]
["","","","Μέτρια","m³/min","6.6"]
["","","","Χαμηλή","m³/min","4.4"]
["","","","Αθόρυβη λειτουργία","m³/min","2.6"]
["","","Θέρμανση","Υψ.","m³/min","10.2"]
["","","","Μέτρια","m³/min","8.4"]
["","","","Χαμηλή","m³/min","6.3"]
["","","","Αθόρυβη λειτουργία","m³/min","3.8"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","54"]
["","Θέρμανση","","","dBA","56"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","38"]
["","","","Μέτρια","dBA","32"]
["","","","Χαμηλή","dBA","25"]
["","","","Αθόρυβη λειτουργία","dBA","19"]
["","Θέρμανση","","Υψ.","dBA","40"]
["","","","Μέτρια","dBA","34"]
["","","","Χαμηλή","dBA","28"]
["","","","Αθόρυβη λειτουργία","dBA","19"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.50"]
["","Αποχέτευση","","","","18"]
["Χειριστήρια","Infrared remote control","","","","ARC466A9"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Batteries","","","","2"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1"]
["","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]
["Σημειώσεις","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]