{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-N"]
[]
[]
[]
[]
["","","","","","RXTM30N2V1B","RXTM40N2V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","49","49"]
["","Ψύξη","","Ονομ.","dBA","48","48"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1"]
["","Ετικέτα πλήρωσης ψυκτικού","","","","1","1"]
["","Πολύγλωσσες ετικέτες των φθοριούχων αερίων του θερμοκηπίου","","","","1","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","0.7","0.7"]
["","GWP","","","","675","675"]
["","Charge","","","kg","1.1","1.1"]
["","Τύπος","","","","R-32","R-32"]
["Κινητ. ανεμ.","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","rpm","450","360"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","rpm","360","360"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","763","763"]
["","","","Βάθος","mm","312","312"]
["","","","Ύψος","mm","551","551"]
["Βάρος","Μονάδα","","","kg","38","38"]
["Power supply","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","(2) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(2) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]