{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLTRH"]
[]
[]
[]
[]
["","","","","WLTRH."]
["Μέγιστος αριθμός εσωτερικών μονάδων που μπορούν να συνδεθούν","","","","0"]
["Μέγιστος αριθμός εξωτερικών μονάδων που μπορούν να συνδεθούν @","","","","0"]
["Περίβλημα","Χρώμα","","","Λευκό"]
["","Κάλυμμα κουμπιών","","","Όχι"]
["","LED Λειτουργίας","Χρώμα","","Πράσινο"]
["Διαστάσεις","Μονάδα","Ύψος","mm","75"]
["","","Πλάτος","mm","60.0"]
["","","Βάθος","mm","25.0"]
["","Μονάδα με στεγανοποίηση","Ύψος","mm","380"]
["","","Πλάτος","mm","305"]
["","","Βάθος","mm","195"]
["Βάρος","Μονάδα","","kg","0.036"]
["Συσκευασία","Υλικό","","","Χαρτόνι"]
["","Βάρος","","kg","0.0084"]
["Θερμοκρασία περιβάλλοντος","Λειτουργία","Ελάχ.","°C","-10"]
["","","Μέγ.","°C","50"]
["","Φύλαξη","Ελάχ.","°C","-10"]
["","","Μέγ.","°C","50"]
["","Θερμοκρασία περιβάλλοντος-=-Σχετική υγρασία <-=-%","","%","100"]
["Εγκατάσταση","","","","Εσωτερική εγκατάσταση"]